Electrical Lighting Controls Schedule

Revision Date Description Created Checked

T1 2 Tender Issue

**Schedule of Equipment – Stand Alone - iLight Solo Applications**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Code** | **Description** | **iLight Series** | **Product Code** | **Image** | **Areas** |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| MB | 10 output, 6 pole marshalling box | iLight Solo | LCC-10 | **Graphical user interface  Description automatically generated** | Open plan offices/meeting rooms |
| PD1 | Absence/Presence detector 230V | iLight Solo | PPAD-C-230V |  | Switching applications |
| PIR lead 1 | For connection to PIR PPAD-C-230V | iLight Solo | SL-6P-4C-3MorSL-6P-4C-5M | A close-up of a headphone  Description automatically generated with low confidence | Suspended ceiling |
| PD2 | DALI Absence/Presence detector 230V | iLight Solo | PPAD-C-DALI-230V |  | DALI dimming applications |
| PIR lead 2 | For connection to PIRPPAD-C-DALI-230V | iLight Solo | SL-6P-5C-3MOrSL-6P-5C-5M | A picture containing cable, connector, adapter  Description automatically generated | Suspended ceiling |
| Luminaire leads | 3,4,5, & 6 core leads | iLight Enterprise / Solo | Various | A picture containing weapon  Description automatically generated | Suspended ceiling |
| Luminaireplugs | Standard & emergency | iLight Enterprise / Solo | Standard ACCPL-6P-01-BEmergency ACCPL-6P-01-R | A picture containing weapon, gun  Description automatically generated | Suspended ceiling |
| HS1 | Full programming Handset | iLight Solo | HHIR-LCD-PROG | A calculator with a screen  Description automatically generated with medium confidence |  |